# **SIGNALS**

## CAR RED – OUTPUT(W) RED LIGHT FOR CARS TO STOP

* CAR YELLOW – OUTPUT(W) YELLOW LIGHT FOR CARS TO PREPARE FOR RED OR GREEN LIGHT
* CAR GREEN – OUTPUT(W) GREEN LIGTH FOR CARS TO START
* PEDESTRIAN RED – OUTPUT(W) RED LIGHT FOR PEDESTRIAN TO STOP CROSSING
* PEDESTRIAN GREEN – OUTPUT(W) GREEN LIGHT PEDESTRIAN TO START CROSSING
* PEDESTRIAN REQUEST- INPUT( R ) BUTTON FOR CROSSING REQUEST
* PEDESTRIAN ANNIMATION ON/OFF - ON FOR WALKING SILUETE ANNIMATION/

OFF FOR STANDING SILUETE ANNIMATION

* PEDESTRIAN SPEAKER-OUTPUT(W) SPEAKER FOR BLIND PEOPLE TO SIGNAL

PEDESTRIAN GREEN LIGHT